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AI-generated content may be incorrect.]Minneapolis Water Works
Monthly Plant Effluent Water Analysis
July 2026

In this report, parts per million is shortened to ppm.
Physical and Chemical Water Quality
	Physical state or chemical
	Plant effluent average value

	Temperature, River Water Average (°C)
	30.1

	Total Organic Carbon (ppm as C)
	5.01

	Total Dissolved Solids (ppm)
	155

	Turbidity (NTU)
	0.05

	Alkalinity-Total (ppm as CaCO3)
	44

	Ammonia Nitrogen (ppm as N)
	0.92

	Total Chloramine Residual (ppm as NH2Cl)
	3.9

	Fluoride-F (ppm as F)
	0.65

	pH
	9.04

	Nitrate - NO3 (ppm as N)
	0.99

	Nitrite - NO2 (ppm as N)
	<0.015

	Phosphate-PO4 (ppm as PO4)
	0.84

	Sulfate - SO4 (ppm as SO4)
	33.4

	Total Hardness (grains per gallon) EDTA method
	5.1

	Total Hardness (ppm as CaCO3) EDTA method
	87



Chemical Water Quality
	Chemical element
	Plant effluent average volume

	Aluminum-Al (ppm as Al)
	0.05

	Arsenic-As (ppm as As)
	Not Detected

	Cadmium-Cd (ppm as Cd)
	Not Detected

	Calcium-Ca (ppm as Ca)
	30.8

	Chloride-Cl (ppm as Cl)
	29.9

	Chromium (ppm as Cr)
	<0.01

	Copper-Cu (ppm as Cu)
	<0.01

	Iron-Fe (ppm as Fe)
	Not Detected

	Lead-Pb (ppm as Pb)
	Not Detected

	Magnesium-Mg (ppm as Mg)
	1.52

	Manganese-Mn (ppm as Mn)
	<0.01

	Silica-Si (ppm as SiO2)
	9.38

	Sodium-Na (ppm as Na)
	17.4

	Zinc-Zn (ppm as Zn)
	<0.01
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